|  |  |
| --- | --- |
| 19”/2® PWR300 Series |  |
|  | |
| |  |  |  | | --- | --- | --- | |  | PWR301 | PWR311 | | Power input | 10-32V DC (max 15A) | 10-32V DC (max 15A) | | Power output | Pass through  Max 10A per port | Pass through  Max 10A per port | | Number of inputs | 1x DC in | 1x DC in | | Number of outputs | 6x DC out | 6x DC out | | Output protection | 10A mechanical circuit breakers | 10A mechanical circuit breakers | | MIL-STD-1275D | No | Yes | | Dimensions (WxDxH) | 220 x 182 x 44 mm  (8,7” x 8,2” x 11,9”) | 220x 300 x 44 mm  (8,7” x 11,9” x 1,7”) | | Weight | 2 kg | 3.5 kg |   **Model Comparison** | |