|  |  |
| --- | --- |
| 19”/2® PWR300 Series |  |
|  |
|

|  |  |  |
| --- | --- | --- |
|  | PWR301 | PWR311 |
| Power input | 10-32V DC (max 15A) | 10-32V DC (max 15A) |
| Power output | Pass throughMax 10A per port | Pass throughMax 10A per port |
| Number of inputs | 1x DC in | 1x DC in |
| Number of outputs | 6x DC out | 6x DC out |
| Output protection | 10A mechanical circuit breakers | 10A mechanical circuit breakers |
| MIL-STD-1275D | No | Yes |
| Dimensions (WxDxH) | 220 x 182 x 44 mm(8,7” x 8,2” x 11,9”) | 220x 300 x 44 mm(8,7” x 11,9” x 1,7”) |
| Weight | 2 kg | 3.5 kg |

**Model Comparison** |